# PyRadio Configuration File

# Player selection
# This is the equivalent to the -u , --use-player command line parameter
# Specify the player to use with PyRadio, or the player detection order
# Example:
#   player = vlc
# or
#   player = vlc,mpv, mplayer
# Default value: mpv,mplayer,vlc
player = mpv,mplayer,vlc

# Default playlist
# This is the playlist to open if none is specified
# You can specify full path to CSV file, or if the playlist is in the
# config directory, playlist name (filename without extension) or
# playlist number (as reported by -ls command line option)
# Default value: stations
default_playlist = stations

# Default station
# This is the equivalent to the -p , --play command line parameter
# The station number within the default playlist to play
# Value is 1..number of stations, "-1" or "False" means no auto play
# "0" or "Random" means play a random station
# Default value: False
default_station = False

# Enable mouse
# If this options is enabled, the mouse can be used to scroll the
# playlist, start, stop and mute the player, adjust its volume etc.
# Mouse integration is highly terminal dependent, that's why it
# is disabled by default.
#
# Default value: False
enable_mouse = True

# Desktop notifications
# If this option is enabled, a Desktop notification will be
# displayed using the notification daemon / service.
# If enabled but no notification is displayed, please refer to
# https://github.com/coderholic/pyradio/desktop-notification.md
# Valid values are:
#   -1: disabled
#    0: enabled (no repetition)
#    x: enabled and repeat every x seconds
#
# Default value: -1
enable_notifications = 0

# Connection timeout
# PyRadio will wait for this number of seconds to get a station/server
# message indicating that playback has actually started.
# If this does not happen (within this number of seconds after the
# connection is initiated), PyRadio will consider the station
# unreachable, and display the "Failed to connect to: [station]"
# message.
#
# Valid values: 5 - 60, 0 disables check
# Default value: 10
connection_timeout = 20

# Force http connections
# Most radio stations use plain old http protocol to broadcast, but
# some of them use https. If this is enabled,  all connections will
# use http; results depend on the combination of station/player.
#
# Valid values: True, true, False, false
# Default value: False
force_http = False

# Default theme
# Hardcooded themes:
#   dark (default) (8 colors)
#   light (8 colors)
#   dark_16_colors (16 colors dark theme alternative)
#   light_16_colors (16 colors light theme alternative)
#   black_on_white (bow) (256 colors)
#   white_on_black (wob) (256 colors)
# If theme is watched for changes, prepend its name
# with an asterisk (i.e. '*my_theme')
# This is applicable for user themes only!
# Default value = 'dark'
theme = blue

# Transparency setting
# If False, theme colors will be used.
# If True and a compositor is running, the stations' window
# background will be transparent. If True and a compositor is
# not running, the terminal's background color will be used.
# Valid values: True, true, False, false
# Default value: False
use_transparency = True

# Calculated color factor
# This is to produce Secondary Windows background color
# A value of 0 dissables it, otherwise it is the factor
# to change (lighten or darken) the base color.
# For more info, please refer to
# https://github.com/coderholic/pyradio#secondary-windows-background
# Valid values: 0-0.2
# Default value: 0
calculated_color_factor = 0

# Playlist management
#
# Specify whether you will be asked to confirm
# every station deletion action
# Valid values: True, true, False, false
# Default value: True
confirm_station_deletion = True

# Specify whether you will be asked to confirm
# playlist reloading, when the playlist has not
# been modified within PyRadio
# Valid values: True, true, False, false
# Default value: True
confirm_playlist_reload = True

# Specify whether you will be asked to save a
# modified playlist whenever it needs saving
# Valid values: True, true, False, false
# Default value: False
auto_save_playlist = True

# Remote Control server
# A simple http server that can accept remote
# connections and pass commands to PyRadio
#
# Valid values:
#   remote_control_server_ip: localhost, LAN, lan
#   remote_control_server_port: 1025-65535
#
# Default value: localhost:9998
#                no auto start
remote_control_server_ip = localhost
remote_control_server_port = 9998
remote_control_server_auto_start = False
