# Alpine Linux dhcp configuration for static IP
# Also manually set DNS in /etc/resolv.conf
# eg.
# nameserver 192.168.0.1
# nameserver 8.8.8.8

auto lo
iface lo inet loopback

auto eth0
iface eth0 inet static
    address 192.168.0.147
    netmask 255.255.255.0
    gateway 192.168.0.1
# For default dynamic IP address
#auto eth0
#iface eth0 inet dhcp
