#!/bin/sh
exec tail -n +3 $0
# This file provides an easy way to add custom menu entries.  Simply type the
# menu entries you want to add after this comment.  Be careful not to change
# the 'exec tail' line above.
#
# DO NOT EDIT THIS FILE
#
# It is automatically generated by grub-mkconfig using templates
# from /etc/grub.d and settings from /etc/default/grub
#

### BEGIN /etc/grub.d/00_header ###
insmod part_gpt
insmod part_msdos
if [ -s $prefix/grubenv ]; then
  load_env
fi
if [ "${next_entry}" ] ; then
   set default="${next_entry}"
   set next_entry=
   save_env next_entry
   set boot_once=true
else
   set default="0"
fi

if [ x"${feature_menuentry_id}" = xy ]; then
  menuentry_id_option="--id"
else
  menuentry_id_option=""
fi

export menuentry_id_option

if [ "${prev_saved_entry}" ]; then
  set saved_entry="${prev_saved_entry}"
  save_env saved_entry
  set prev_saved_entry=
  save_env prev_saved_entry
  set boot_once=true
fi

function savedefault {
  if [ -z "${boot_once}" ]; then
    saved_entry="${chosen}"
    save_env saved_entry
  fi
}

function load_video {
  if [ x$feature_all_video_module = xy ]; then
    insmod all_video
  else
    insmod efi_gop
    insmod efi_uga
    insmod ieee1275_fb
    insmod vbe
    insmod vga
    insmod video_bochs
    insmod video_cirrus
  fi
}

terminal_output console
if [ x$feature_timeout_style = xy ] ; then
  set timeout_style=hidden
  set timeout=1
# Fallback hidden-timeout code in case the timeout_style feature is
# unavailable.
elif sleep --interruptible 1 ; then
  set timeout=0
fi
### END /etc/grub.d/00_header ###

### BEGIN /etc/grub.d/10_linux ###
menuentry 'Arch Linux' --class arch --class gnu-linux --class gnu --class os $menuentry_id_option 'gnulinux-simple-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
	load_video
	set gfxpayload=keep
	insmod gzio
	insmod part_gpt
	insmod fat
	set root='hd0,gpt1'
	if [ x$feature_platform_search_hint = xy ]; then
	  search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt1 --hint-efi=hd0,gpt1 --hint-baremetal=ahci0,gpt1  5977-60ED
	else
	  search --no-floppy --fs-uuid --set=root 5977-60ED
	fi
	echo	'Loading Linux linux-zen ...'
	linux	/vmlinuz-linux-zen root=UUID=71dcad6d-3c93-473d-ad60-0cea0d6d379c rw rootflags=subvol=@arch       quiet loglevel=3 rd.udev.log_level=3     rd.vconsole.keymap=colemak         cryptdevice=/dev/disk/by-label/CRYPTROOT:main         root=/dev/disk/by-label/ROOT         rootflags=rw,noatime,compress=zstd,subvol=//@arch
	echo	'Loading initial ramdisk ...'
	initrd	/intel-ucode.img /initramfs-linux-zen.img
}
submenu 'Advanced options for Arch Linux' $menuentry_id_option 'gnulinux-advanced-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
	menuentry 'Arch Linux, with Linux linux-zen' --class arch --class gnu-linux --class gnu --class os $menuentry_id_option 'gnulinux-linux-zen-advanced-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
		load_video
		set gfxpayload=keep
		insmod gzio
		insmod part_gpt
		insmod fat
		set root='hd0,gpt1'
		if [ x$feature_platform_search_hint = xy ]; then
		  search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt1 --hint-efi=hd0,gpt1 --hint-baremetal=ahci0,gpt1  5977-60ED
		else
		  search --no-floppy --fs-uuid --set=root 5977-60ED
		fi
		echo	'Loading Linux linux-zen ...'
		linux	/vmlinuz-linux-zen root=UUID=71dcad6d-3c93-473d-ad60-0cea0d6d379c rw rootflags=subvol=@arch       quiet loglevel=3 rd.udev.log_level=3     rd.vconsole.keymap=colemak         cryptdevice=/dev/disk/by-label/CRYPTROOT:main         root=/dev/disk/by-label/ROOT         rootflags=rw,noatime,compress=zstd,subvol=//@arch
		echo	'Loading initial ramdisk ...'
		initrd	/intel-ucode.img /initramfs-linux-zen.img
	}
	menuentry 'Arch Linux, with Linux linux-zen (fallback initramfs)' --class arch --class gnu-linux --class gnu --class os $menuentry_id_option 'gnulinux-linux-zen-fallback-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
		load_video
		set gfxpayload=keep
		insmod gzio
		insmod part_gpt
		insmod fat
		set root='hd0,gpt1'
		if [ x$feature_platform_search_hint = xy ]; then
		  search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt1 --hint-efi=hd0,gpt1 --hint-baremetal=ahci0,gpt1  5977-60ED
		else
		  search --no-floppy --fs-uuid --set=root 5977-60ED
		fi
		echo	'Loading Linux linux-zen ...'
		linux	/vmlinuz-linux-zen root=UUID=71dcad6d-3c93-473d-ad60-0cea0d6d379c rw rootflags=subvol=@arch       quiet loglevel=3 rd.udev.log_level=3     rd.vconsole.keymap=colemak         cryptdevice=/dev/disk/by-label/CRYPTROOT:main         root=/dev/disk/by-label/ROOT         rootflags=rw,noatime,compress=zstd,subvol=//@arch
		echo	'Loading initial ramdisk ...'
		initrd	/intel-ucode.img /initramfs-linux-zen-fallback.img
	}
	menuentry 'Arch Linux, with Linux 5.15.32_1' --class arch --class gnu-linux --class gnu --class os $menuentry_id_option 'gnulinux-5.15.32_1-advanced-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
		load_video
		set gfxpayload=keep
		insmod gzio
		insmod part_gpt
		insmod fat
		set root='hd0,gpt1'
		if [ x$feature_platform_search_hint = xy ]; then
		  search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt1 --hint-efi=hd0,gpt1 --hint-baremetal=ahci0,gpt1  5977-60ED
		else
		  search --no-floppy --fs-uuid --set=root 5977-60ED
		fi
		echo	'Loading Linux 5.15.32_1 ...'
		linux	/vmlinuz-5.15.32_1 root=UUID=71dcad6d-3c93-473d-ad60-0cea0d6d379c rw rootflags=subvol=@arch       quiet loglevel=3 rd.udev.log_level=3     rd.vconsole.keymap=colemak         cryptdevice=/dev/disk/by-label/CRYPTROOT:main         root=/dev/disk/by-label/ROOT         rootflags=rw,noatime,compress=zstd,subvol=//@arch
		echo	'Loading initial ramdisk ...'
		initrd	/intel-ucode.img /initramfs-5.15.32_1.img
	}
	menuentry 'Arch Linux, with Linux 5.15.30_1' --class arch --class gnu-linux --class gnu --class os $menuentry_id_option 'gnulinux-5.15.30_1-advanced-71dcad6d-3c93-473d-ad60-0cea0d6d379c' {
		load_video
		set gfxpayload=keep
		insmod gzio
		insmod part_gpt
		insmod fat
		set root='hd0,gpt1'
		if [ x$feature_platform_search_hint = xy ]; then
		  search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt1 --hint-efi=hd0,gpt1 --hint-baremetal=ahci0,gpt1  5977-60ED
		else
		  search --no-floppy --fs-uuid --set=root 5977-60ED
		fi
		echo	'Loading Linux 5.15.30_1 ...'
		linux	/vmlinuz-5.15.30_1 root=UUID=71dcad6d-3c93-473d-ad60-0cea0d6d379c rw rootflags=subvol=@arch       quiet loglevel=3 rd.udev.log_level=3     rd.vconsole.keymap=colemak         cryptdevice=/dev/disk/by-label/CRYPTROOT:main         root=/dev/disk/by-label/ROOT         rootflags=rw,noatime,compress=zstd,subvol=//@arch
		echo	'Loading initial ramdisk ...'
		initrd	/intel-ucode.img /initramfs-5.15.30_1.img
	}
}

### END /etc/grub.d/10_linux ###

### BEGIN /etc/grub.d/20_linux_xen ###

### END /etc/grub.d/20_linux_xen ###

### BEGIN /etc/grub.d/30_os-prober ###
### END /etc/grub.d/30_os-prober ###

### BEGIN /etc/grub.d/30_uefi-firmware ###
menuentry 'UEFI Firmware Settings' $menuentry_id_option 'uefi-firmware' {
	fwsetup
}
### END /etc/grub.d/30_uefi-firmware ###

### BEGIN /etc/grub.d/40_custom ###
# This file provides an easy way to add custom menu entries.  Simply type the
# menu entries you want to add after this comment.  Be careful not to change
# the 'exec tail' line above.
### END /etc/grub.d/40_custom ###

### BEGIN /etc/grub.d/41_custom ###
if [ -f  ${config_directory}/custom.cfg ]; then
  source ${config_directory}/custom.cfg
elif [ -z "${config_directory}" -a -f  $prefix/custom.cfg ]; then
  source $prefix/custom.cfg
fi
### END /etc/grub.d/41_custom ###
